**********************************************************************

ADDITIONAL NOTES ABOUT USING MWAVE IN Windows 95

Mwave Release 2.3

(c) 1996, IBM Corp.
11:07 a.m., July 23, 1996
**********************************************************************

--------------------
INTRODUCTION
--------------------

This document provides information to help you properly run Mwave appli-
cations in Microsoft Windows 95.  A list of "frequently-asked questions"
(FAQs) presents answers to questions or problems you may encounter while
working with the Mwave product. Other topics include solutions to compat-
ibility issues and installation problems, as well as additional technical
notes.

-------------------------
Windows 95 Compatibility
-------------------------

Mwave has been tested and proven compatible with Microsoft Windows 95.
For additional compatibility information, refer to section 4.0 below.

-----------------------
Printing This Document
-----------------------

To print this document from Windows 95, highlight the document in Windows
Explorer and choose the Print command from the File menu.

------------------------
Other Helpful Documents
------------------------

The following online document provides additional information about Mwave
Windows applications:

       MWHELP.HLP    This help file presents a general overview of all
                     the components in Mwave.  To view this
                     file from Windows 95, click Start,
                     point to Programs, Mwave, and click Mwave
                     Help.

======================================================================
CONTENTS
======================================================================

    1.0  BEFORE YOU CALL FOR HELP

    2.0  INSTALLATION NOTES

        2.1  Installing Mwave for Windows 95
        2.2  Installing MIDI Samples for Windows 95
        2.3  Turning Mwave OFF and ON in DOS
        2.4  Selective Uninstall of Mwave Features in Windows 95

    3.0  FREQUENTLY-ASKED QUESTIONS (FAQs)

        3.1  FAQs about the Mwave Modem
        3.2  FAQs about Mwave FAX Capabilities
        3.3  FAQs about Mwave's Speaker Phone Capabilities
        3.4  FAQs about Mwave Audio Features
        3.5  FAQs about Mwave's Telephone Country Selection Utility
        3.6  FAQs about Mwave's Sound Blaster Emulation
        3.7  FAQs about Mwave and Loading Windows 95

    4.0  COMPATIBILITY

        4.1  Communications (Modem) Applications
        4.2  Windows FAX Applications
        4.3  DOS FAX Applications
        4.4  Memory Problems with Windows and DOS TSRs
        4.5  Other Applications and Mwave

    5.0  OTHER TECHNICAL NOTES

        5.1  Recommendations for Optimum Mwave Modem Performance
        5.2  Audio/MIDI Technical Notes
        5.3  Sound Blaster Technical Notes
        5.4  Notes about the Mwave Modem
        5.5  Notes about DOS Mode Support

======================================================================
1.0  BEFORE YOU CALL FOR HELP
======================================================================

Before you call the technical support group, please read this entire doc-
ument for any installation, configuration, or compatibility information.
Also, the FAQs provide a good basis for answering most common questions.

If the document does not provide a solution and you need to contact tech-
nical support, please have your computer running. For faster service,
have the following information ready for our technical support personnel:

o   Make and model of your computer
o   Mwave software version number
o   Names and version numbers of application software you are running
o   Contents of your \WINDOWS\DOSSTART.BAT, AUTOEXEC.BAT, and CONFIG.SYS
    files (You can either print the files, or have access to an editor to
    view them.)

======================================================================
2.0  INSTALLATION NOTES
======================================================================

No installation errors have been reported. Please contact Product Support
if you encounter a problem during installation of the Mwave product.

----------------------------------------------------------------------
2.1  Installing Mwave for Windows 95
----------------------------------------------------------------------

1.  Power off your machine.

2.  Disconnect the power cord.

3.  Install the Mwave card.

4.  Reconnect the power cord and start up your PC.

5.  When Windows 95 is running, place Mwave installation disk #1 in the
    A: drive.

6.  Click the START icon at the bottom of the screen.

7.  Click RUN and type A:UINSTALL in the text entry box.  Mwave code
    installation begins.  Follow the install instructions.

8.  When the Mwave installation is complete, reboot Windows 95.

9.  When Windows 95 is rebooted, open the Control Panel and click ADD NEW
    HARDWARE.

    a.  Click NEXT
    b.  Click NO
    c.  Select OTHER devices in the "Hardware Types" menu
    d.  Click NEXT
    e.  Locate "IBM" in the "Manufactures" list
    f.  In the "Models" list select the MWAVE OEM DSP Adapter
    g.  Click NEXT
    h.  Click FINISH.  Windows 95 begins setting up the new Mwave hard-
        ware.

10. When Windows 95 locates the base hardware it instructs you to reboot.

    NOTE:  Be sure to turn the machine off at this point or the PALs on
    the MWAVE card will not set up properly.

11. As Windows 95 reboots, it locates children devices of the Mwave DSP.
    When this process is complete, Mwave is ready to run and you should
    hear system sounds.

NOTE:  Non-US users must run the Country Selection Application AFTER
Mwave installation and reboot.  Reboot again after running the Country
Selection Application.

----------------------------------------------------------------------
2.2  Installing MIDI Samples for Windows 95
----------------------------------------------------------------------

To install the Mwave MIDI Samples:

1.  Insert disk 1 of the Advanced MIDI Samples in your floppy drive.
2.  Click Start
3.  Click Run
4.  Type a:\setup in the OPEN window
5.  Click OK
6.  Choose the path in which to install the samples.  We recommend using
    the default path.
7.  Insall the Advanced MIDI Samples and allow the Windows synthesizer to
    use this sample set when prompted.
8.  Do NOT reboot at this time.
9.  Insert Disk 1 of the EMU MIDI Samples.
10. Click Start
11. Click Run
12. Type a:\setup in the OPEN window
13. Click OK
14. Choose the path in which to install the samples.  We recommend using
    the default path.
15. Install the EMU MIDI Samples.  Use this sample set for the Mwave DOS
    synthesizer ONLY.  Do NOT use this sample set for the Mwave Windows
    synthesizer.
16. Reboot your machine when the installation completes.

----------------------------------------------------------------------
2.3  Turning Mwave OFF and ON in DOS
----------------------------------------------------------------------

NOTE:  The following section applies when you shutdown or boot to:

    -   Native DOS only from Windows 3.x
    -   MS-DOS mode only from Windows 95

If you are running Mwave under DOS only, type the following commands from
the DOS prompt:

o   MWAVE OFF--To turn Mwave off
o   MWAVE START--To re-initialize Mwave and begin a fresh session without
    rebooting
o   MWAVE ON--To restart Mwave with the same settings as the previous
    session
o   FASTCFG--To change application types

If you use MWAVE OFF to stop Mwave and then use FASTCFG to restart Mwave,
you must change the application type.

----------------------------------------------------------------------
2.4  Selective Uninstall of Mwave Features in Windows 95
----------------------------------------------------------------------

To use a different audio, modem, or Sound Blaster card than provided by
Mwave, you must uninstall the Mwave feature before installing the substi-
tute card.  To uninstall Mwave features, perform the following steps:

o   Click START
o   Point to SETTINGS
o   Click Control Panel
o   Double-click System
o   Click the Device Manager tab
o   Click the "Plus" sign next to the device you want to uninstall
o   Click on the device
o   Click Properties
o   Click on the check next to "Original Configuration (Current)" in the
    Device Usage box. This disables the device.
o   Click OK
o   Click Close
o   Reboot the system

NOTE:  To reinstall the device, simple replace the check in the Device
Usage box.

======================================================================
3.0  FREQUENTLY-ASKED QUESTIONS (FAQs)
======================================================================

This section contains answers to questions about certain features and
capabilities provided by Mwave applications.

----------------------------------------------------------------------
3.1  FAQs about the Mwave Modem
----------------------------------------------------------------------

Q: What should I do if I answer an incoming phone call with the handset
   and then discover that the call is a fax or modem transmission?

A: Fax machines and modems are usually set up to call back several times
   if they fail to make a connection.  Therefore, hang up and, when the
   fax machine or modem calls back, allow the PC to answer the call.
   Mwave enables the PC to discriminate (determine the call type) and
   either pass the call to the open fax or modem application, or take a
   message for a voice call.

Q: Why don't I hear modem sounds when I run the Microsoft Hardware
   Compatability Test (MHCT) for the modem?

A: The MHCT tests the modem's M2 command.  M2 is the command to keep the
   speakers on all the time.  Mwave's DSP maps the M2 command to M1,
   which commands no sound when the modem is connected.  Therefore, no
   sound is heard when tested.

Q: Why am I unable to telegame from a Windows 95 DOS session?

A: Telegaming in a Windows 95 DOS session requires a limited modem speed
   of 14.4 kbps (V.32) and the modem default speed is 28.8 kbps.  To
   enable telegaming within a DOS session, set the modem speed to 14.4
   kbps.  To change the modem speed:

   o   Open the Mwave Modem.
   o   Click Options.
   o   Click Settings.
   o   Select 14400 (V.32 bis).
   o   Click OK.

   NOTE:  If the options in the Settings window are greyed-out, your
   modem is connected; it must be disconnected for you to change the
   modem speed.

Q: What settings do I need to use when I install a communications appli-
   cation (such as ProComm or CrossTalk)?

A: Your communications software requires that you provide a modem type, a
   baud rate (i.e, the speed of your modem), and the COM port to which
   the modem is attached.

   The chart below describes settings required by Mwave:

       To set this...        Select highest ranking available setting...
       -------------------------------------------------------------------
       The Modem type        1. Mwave modem
                             2. Generic Hayes-type modem
                             3. User-defined modem
                             4. Hayes SmartModem 2400
                             5. Hayes modem
                             6. Hayes compatible modem
                             7. Other (Note: If you select a modem of
                                   type "Other," you must include the
                                   proper modem initialization string.
                                   For most applications, the
                                   initialization string "AT&F" will
                                   work. See the Mwave Modem online
                                   help for more information.)

       Baud Rate             57,600 bps, or the maximum setting offered
                             by your communications software.

       COM Port              COM 1 (If your mouse is assigned this port,
                                    use COM 2.)

Q: What can I do if my 300 baud modem connections are unreliable?

A: Use the next higher setting (or baud rate) and try again. It is recom-
   mended that you use the highest possible setting of your Mwave Modem.

Q: What port speed should I use when I connect my modem at 2400 bps?

A: If you attempt to force the modem to connect at 2400 bps by setting
   the port speed to that value, the connection may not be made or it may
   fall back to 2400 nECL or 1200.  To avoid this problem, set the port
   speed to a higher value.

Q: What host application transfer protocol is recommended for best Mwave
   Modem performance?

A: For best throughput when sending or receiving data, select the
   highest-ranking available transfer protocol listed here.

   1.  ZMODEM
   2.  Kermit-95
   3.  Ymodem-G
   4.  TEXT
   5.  ASCII
   6.  XMODEM (only as a last resort)

   For more information, see Section 5.1  Recommendations for Optimum
   Mwave Modem Performance.

----------------------------------------------------------------------
3.2  FAQs about Mwave FAX Capabilities
----------------------------------------------------------------------

Q: What setting should I use for the "fax/modem type" when I set up my
   Class 2 FAX software to work with Mwave if "Mwave Modem" isn't listed
   as an option?

A: For all FAX applications, if "Mwave Modem" is not listed, select
   "Generic Class 2" or some comparable label from the application's list
   of supported fax/modems.

Q: What should I do if I answer an incoming phone call with the handset
   and then discover that the call is a fax or modem transmission?

A: See first Q & A in the above section, FAQs About the Mwave Modem.

Q: What are Mwave's fax restrictions?

A: Mwave supports fax transmissions of monochrome text and images up to 8
   1/2 inches wide (A4 width).  Mwave does not support B4 width trans-
   missions.

----------------------------------------------------------------------
3.3  FAQs about Mwave's Speaker Phone Capabilities
----------------------------------------------------------------------

Q: How do I prevent the speaker phone from terminating a telephone call
   when my computer is set to automatically suspend after a period of
   time with no keyboard activity?

A: To avoid having your telephone calls terminated when your computer
   uses the Suspend/Resume Power Management feature, double-click the
   Power icon in the Setup group Start/Settings/Control Panel to choose a
   setup that does not include activation of the suspend mode when you
   don't use the mouse or keyboard.

Q: When the Phoenix Message Center records an incoming call, how do I
   prevent it from appending a dial tone to the end of the message?

A: The Phoenix Message Center's answering system requests that each
   caller ends his/her message by pressing the "#" key before hanging up.
   The calls you receive with "appended dial tones" occur when the caller
   does not press #.

----------------------------------------------------------------------
3.4  FAQs about Mwave Audio Features
----------------------------------------------------------------------

Q: Why can't I play a compact disc through Windows 95's "My Computer"?

A: Windows 95 must have its CD Player installed before you can play CDs
   through My Computer. To make sure the Windows 95 CD Player is loaded:

   1.  Select Settings from the Start menu, then select Control Panel.
   2.  Double-click the Add/Remove Program icon.
   3.  Select the Windows Setup tab.
   4.  Select Multimedia.
   5.  Select the CD Player check box, then click OK.

Q: Why don't I hear any sound when playing a MIDI file with Windows 95's
   Media Player?

A: You won't hear any sound when playing a MIDI file if your MIDI drivers
   have not been configured for Mwave. To make sure that Mwave is prop-
   erly configured:

   1.  Select Settings from the Start menu.
   2.  Select the Control Panel.
   3.  Select Multimedia.  From the multimedia screen, select "MIDI".
       Select "Single instrument" and highlight "Mwave MIDI Synthesizer".

Q: Why do I receive an error message when I try to play an Mwave
   Synthesizer Samples .WAV file in an audio application?

A: The Mwave Synthesizer uses samples in the form of *.WAV files
   installed on the hard disk to play music.  These WAV files are
   intended solely for use by the synthesizer and are formatted correctly
   for this purpose.  However, if for some reason a user tries to use an
   audio application to play the *.WAV files individually, the applica-
   tion may respond with an error message.  This does not indicate a
   problem in using the files for their intended purpose.

Q: Why doesn't the sound playback when I make a mono recording?

A: Mono recordings often record on only one stereo channel.  Therefore,
   make sure the balance sliders are at the center setting when recording
   and replaying.

Q: What should I do when I receive a "WinDAT error" when I try to play or
   record a .WAV file through AudioStation?

A: The AudioStation Mixer cannot handle Wave (.WAV) files. You can use
   the Windows 95 Media Player for Wave playback or Windows 95's Sound
   Recorder for both playback and record.

Q: How can I prevent the noise in my 8 bit recordings?

A: An 8 bit recording is naturally noisy.  To reduce the noise level of
   your recording, use 16 bit recording.

Q: How do I get Sound Blaster games to run after a suspend/resume when it
   has been running with MIDI?

A: Stopping MIDI will not enable Sound Blaster games to run correctly.
   Instead, close and then reopen the Sound Blaster application.

Q: Sound Blaster games run after a suspend/resume but my Telephone
   Answering Machine (TAM) cannot receive calls.  How do I reactivate the
   TAM?

A: Close and then reopen the Sound Blaster application.

Q: How do I restore the sound to games such as DOOM or DOOM II running in
   a Windows 95 DOS session after a suspend/resume?

A: Close and then reopen the game application.

Q: How do I enable both Sound Blaster music and sounds in games such as
   DOOM II telegaming in Windows 95 DOS-mode?

A: You must change the Mwave modem setting to V.32bis (14,400).  To
   change the setting:

   1.  Click START
   2.  Point to PROGRAMS and then MWAVE
   3.  Click Mwave Modem
   4.  Click OPTIONS on the menu bar and then SETTINGS...
   5.  Click 14400 (V.32bis)
   6.  Click OK

Q: Why am I unable to telegame?

A: When audio mixer options are selected, they consume the DSP resources
   necessary to telegame, even when the mixer is off.  Therefore, to
   enable telegaming you must disable the mixer options such as Effects
   and Qsound.

Q: Why do I hear pauses when I play an audio wave (.WAV) recording from a
   floppy diskette?

A: These pauses during playback occur due to the slower rate of data
   transfer from the diskette. To fix the problem, copy the wave (.WAV)
   file to your hard disk.

Q: Why does my .WAV file I just recorded sound "broken"?

A: "Broken" or discontinuous sound is often the result of either the
   slower data transfer rate from a floppy drive, or you recorded the
   .WAV file to a drive that is compressed (using DriveSpace,
   DoubleSpace, or Stacker). In both cases, the playback application
   cannot receive data fast enough and, as a result, you hear the gaps in
   the transaction.

   To fix this problem, you can:

   o   Record the .WAV file to a fixed disk (i.e., C: ).
   o   Lower the record rate to 22 KHz or 11 KHz, change to 8 bit, and/or
       change to mono sound. Most applications allow you to adjust these
       parameters, and less taxing record rates may solve the problem.
   o   If you use a disk compression program (such as DriveSpace,
       DoubleSpace, or Stacker), direct the recorded data to an uncom-
       pressed drive. This way, the computer can process the sound
       without taking the time to uncompress/compress the information.

   Refer to Section 5.2  Audio/MIDI Technical Notes for additional tech-
   nical information.

Q: Why don't I hear sounds from my game or CD when the Mwave Modem is
   also running?

A: Mwave manages the workload of the digital signal processor, the device
   that allows you to play sound, use telephony, etc. If you don't hear
   sounds from your DOS game or CD, it is likely that Mwave is using the
   modem to send a file or has set the modem to answer the telephone.

   Wait for these other tasks to finish. You should then hear the sounds
   from your game or CD.

Q: Why does the volume on 8 bit recordings seem softer than 16 bit
   recordings?

A: Most prerecorded 8 bit wave files, like those included with applica-
   tions or Windows, are compressed to improve their signal-to-noise
   (S/N) ratio.  These compressed files are much louder than the uncom-
   pressed audio (wave, synthesizers, MPEG) in the system.

   To compensate for loud prerecorded 8 bit audio, Mwave tasks reduce the
   playback level of all 8 bit recordings.  The volume reduction is done
   with 16 bit precision, so the S/N ratio is NOT reduced.  The reduced
   and compressed 8 bit audio plays slightly louder than typical uncom-
   pressed 16 bit audio, and slightly reduces the volume of uncompressed
   8 bit audio.

Q: What happens if I change the input source of the mixer during
   recording?

A: Changing the input source results in muting of the audio. If you inad-
   vertently do this, restart Windows to recover.

Q: How do I stop feedback from occurring when I use my microphone?

A: Lower the peak levels for playback and record for your microphone.

   1.  Click Start, point to Programs, Mwave, and click Audio Control.
   2.  Click on the MIC button.
   3.  Click and drag the microphone (MIC) slide controls to a lower
       level.
   4.  Resume using the microphone.

   (Note:  When the play pushbutton is selected, make sure that the
   microphone check box is not selected.)

----------------------------------------------------------------------
3.5  FAQs about Mwave's Telephone Country Selection Utility
----------------------------------------------------------------------

Q: What is Country Selection?

A: The Mwave Telephone Country Selection program is used to set country
   specific parameters for Mwave telephony functions including Modem,
   FAX, speakerphone, and Telephone Answering Machine.  The Mwave tele-
   phony drivers use the Country selection information to permit reliable
   and safe connection to the appropriate telephone network.

      **********
       WARNING:    Improper selection of the telephone network may cause
      **********   unreliable operation.

----------------------------------------------------------------------
3.6  FAQs about Mwave's Sound Blaster Emulation
----------------------------------------------------------------------

Q: What sound card does Mwave emulate?

A: Mwave emulates both a Sound Blaster 1.5 (SB) card and a Sound Blaster
   Pro (SB Pro) card.

See additional information in Section 5.3  Sound Blaster Technical Notes
in this file.

----------------------------------------------------------------------
3.7  FAQs about Mwave and Loading Windows 95
----------------------------------------------------------------------

Q: Why can't I open Windows after receiving the following message:

       "Mwave Warning:  Mwave has detected a memory condition that may
       adversely effect Windows operation.  Windows will not be started.
       Restarting your machine may solve this problem.  If this message
       displays again, read \MWW\README.TXT"

A: This message typically calls attention to memory resources used by
   Mwave and DOS "terminate and stay resident" (TSR) programs, such as
   DOSKEY. To avoid the warning message and start Windows, you can:

   o   Make sure that Mwave is loaded after the TSRs by verifying that
       the "CALL MWAVE START" statement in your AUTOEXEC.BAT file follows
       all calls to load TSR programs.  In addition, the "CALL MWAVE
       START" statement must precede the lines that call HWCHECK and
       PS1START.BAT.

   For additional information on the memory error condition message you
   receive when starting Windows, see Section 4.4  Memory Problems with
   Windows and DOS TSRs.

======================================================================
4.0  COMPATIBILITY
======================================================================

Read through this section if you have any problems with a specific appli-
cation working with Mwave.

----------------------------------------------------------------------
4.1  Communications (Modem) Applications
----------------------------------------------------------------------

o   Connecting to Prodigy

    When attempting to use the Mwave Modem to connect to Prodigy using a
    2400 bps Y (Tymnet) connection, the connection fails.  Contact
    Prodigy support for assistance in solving this problem.

o   Microsoft Mail 3.2

    Microsoft Mail 3.2 fails to connect when using the Mwave modem.  The
    suggested fix from Microsoft is to add the line "exclusive=0" under
    the {SFSremote} heading in \WINDOWS\MSMAIL.INI.

o   Windows for Workgroups 3.11

    The Remote Access Support (RAS) doesn't recognize the connected
    response from the Mwave modem. The IBM Personal Computer Company
    (PCC) Bulletin Board Service (BBS) provides a MODEM.INF file with the
    correct Mwave information. You should obtain this file and add the
    information to the \WINDOWS\SYSTEM\MODEM.INF file.

----------------------------------------------------------------------
4.2  Windows FAX Applications
----------------------------------------------------------------------

Mwave Class 2 Fax is compatible with the following Windows Fax applica-
tions:

o   Delrina's WinFax Lite version 3.0 and WinFax Pro version 3.0
o   Delrina's WinFax Pro version 4.0
o   BIT Software's BitFax Pro version 3.07
o   Cheyenne's Bitware Lite version 3.22
o   Trio's Data/Fax Lite version 4.1E
o   Trio's Data/Fax
o   Microsoft's Exchange (Windows 95 Fax) version 4.0.410.59
o   Phoenix Technologies' Eclipse Fax version 6.0
o   Hayes's SmartCom Fax version 1.01B
o   Smith Micro's QuickLink version II 1.4.3
o   Smith Micro's QuickLink Gold version 1.2
o   Sofnet's FaxWorks Pro version 3.0

The following applications are not currently compatible with Mwave Class
2 Fax:

o   Hayes's SmartCom Data/Fax Pro version 1.0A
o   BIT Software's BitFax for Windows version 2.09D
o   Datastorm's ProComm Plus for Windows Fax version 2.00
o   Datastorm's ProComm Plus for Windows versions 2.10 and 2.11
o   Microsoft's Windows for Workgroups Fax version 3.11
o   Delrina's WinFax Lite version 2.0

The following items provide specific information about the fax applica-
tions mentioned above.

o   Delrina's WinFax Pro version 4.0

    If you are installing WinFax Pro 4.0 as a new application, you may
    encounter the following questions and error messages.

    Under Windows 95, installation may stop and inform you of the
    detection of a Windows desktop other than "progman."  You will be


    instructed to exit Windows and use "progman" instead.  Do NOT discon-
    tinue the installation.  Select "Continue" and proceed.  You will
    also be given the opportunity to change the COM driver and FIFO
    parameters.  Select "No" when asked if you want the system to make
    these changes to the \WINDOWS\SYSTEM.INI file.

    The WinFax Pro 4.0 installation prompts you to test the Fax modem.

    -   If you select "Yes," the message "Unable to communicate with
        fax/modem - unknown device" appears.
    -   Select "No" and continue.
    -   From the Fax/Modem Setup screen:
        1.  Set the modem type to Class2
        2.  Select the proper COM port
        3.  Do not change the initialization strings
    -   The message "Setup cannot communicate with the fax device con-
        nected to your COM port.  Do you want to continue?" appears.
    -   Select "Yes."
    -   When asked if you want to make \WINDOWS\SYSTEM.INI file changes,
        select "No."

    The Mwave Fax modem is now properly installed.

o   Phoenix Technologies' Eclipse Fax version 6.0

    Using an editor (such as Notepad), modify the {MODEM} section of the
    \WINDOWS\E-FAX.INI file by changing "Priority FAX=1" to "Priority
    FAX=0"

    When you exit Eclipse, there is a short delay and the message "The
    Modem is not responding" appears.  Ignore this message.

o   Hayes's SmartCom Fax version 1.01B

    You must select the PCMCIA 144/144 FAX modem in the
    Utilities/Hardware configuration dialog box to use Mwave with this
    application.

o   Smith Micro's QuickLink II 1.4.3 and QuickLink Gold 1.2

    When started, QuickLink returns the error message: "Unable to ini-
    tialize modem!  Check modem and/or baud rate setting, then select
    OK."  Ignore this message and select OK.

    The main QuickLink application panel must be displayed in order to
    receive a Fax.

o   Sofnet's FaxWorks Pro version 3.0

    Using an editor (such as Notepad), modify the {MODEM} section of the
    \WINDOWS\FAXWORKS.INI file by changing "Priority FAX=1" to "Priority
    FAX=0"

    When you exit FaxWorks, there is a short delay and the message "Modem
    not responding" appears.  Ignore this message.

General Usage Note:  Many Fax applications offer a custom communications
(COM) driver that may improve Fax transmission speeds.  Mwave uses the
Windows default COM driver when testing these applications.  If a tested
application does not perform, verify that the Windows default COM driver
statement, "comm.drv=comm.drv", is in the {boot} section of the
\WINDOWS\SYSTEM.INI file.  (NOTE: You can use an editor such as Notepad.)

Problems may occur because an applications COM driver is not compatible
with other applications.  In addition, some applications will not give
you the opportunity to change a non-default COM driver, regardless of
compatibility.

----------------------------------------------------------------------
4.3  DOS FAX Applications
----------------------------------------------------------------------

Mwave Class 2 fax is compatible with the following DOS Fax applications:

o   Delrina's DOS Fax Lite version 3.0
o   Delrina's DOS Fax Pro version 2.0
o   Cheyenne's BitFax version 4.05A

The following items provide specific information about the fax applica-
tions mentioned above.

o   Delrina's DOS Fax Pro version 2.0

    The Mwave modem must be running before initializing and using DOS Fax
    Pro.

    NOTE:  The Terminate and Stay Resident Programs (TSRs), added to the
    AUTOEXEC.BAT by Delrina's DOS Fax Pro installation, can cause con-
    flicts in Mwave's ability to send and receive faxes.

o   Cheyenne's BitFax version 4.05A

    Each time you start BitFax, send a fax before attempting to receive
    faxes.  This ensures that BitFax can receive Class 2 faxes from the
    Mwave modem.

Delrina's DOS Fax Lite version 2.00 is not currently compatible with
Mwave Class 2 Fax.

----------------------------------------------------------------------
4.4  Memory Problems with Windows and DOS TSRs
----------------------------------------------------------------------

Loading programs such as DOS TSRs (e.g. DOSKEY) in memory after Mwave
loads may result in a memory error condition and prevent Windows from
starting. There are three ways you can get past the message and start
Windows.

o   To start Windows in most general purpose situations:

    Load Mwave last, after all other items, for it to function properly.
    Check the contents of your AUTOEXEC.BAT file to make sure Mwave loads
    last:

    1.  Open the AUTOEXEC.BAT file with an editor.
    2.  Verify that "CALL MWAVE START" follows all calls to TSR programs.
        Also, make sure "CALL MWAVE START" precedes the statements that
        call HWCHECK and PS1START.BAT.
    3.  Restart your computer.

o   To start Windows after invoking or using a DOS TSR:

    If you invoke certain programs (such as TSRs) in DOS before you start
    Windows, you may encounter memory errors. To avoid these memory prob-
    lems, you must restart your PC before launching Windows.

o   To override the problem and start Windows without unloading TSRs:

    In some situations, you may want to continue with Windows while the
    TSRs consume memory resources. If your PC has more than 8 MB of RAM,
    this should not pose a problem. If your PC has less than 8 MB of RAM,
    you may experience slower performance from Windows.

----------------------------------------------------------------------
4.5  Other Applications and Mwave
----------------------------------------------------------------------

o   Lotus Notes 3.x

    Lotus Notes 3.x does not properly recognize the Mwave modem. Lotus
    does not include an .MDM file that describes the Mwave commands and
    responses.

    To fix this problem, obtain a copy of the MWAVE.MDM file from the PCC
    BBS and add it to the \NOTES directory. Follow these steps:

    1.  Start Lotus Notes 3.x.
    2.  Select the modem configuration. The list of choices should now
        include the Mwave modem.
    3.  Choose the Mwave modem from the list.
    4.  Return to Notes and use as you usually would.

o   Windows 95 Volume Control

    The Mwave Audio Control and the Windows 95 Volume Control applica-
    tions are not synchronized.  Using both controls simultaneously
    results in incorrect settings.  In order to avoid this situation,
    operate only one audio controller.  Microsoft is investigating this
    Windows 95 device driver problem.

o   Windows 95 Phone Dialer

    In order to talk through Windows 95's Phone Dialer with Mwave, you
    must attach a handset via the splitter plug (shipped with the Mwave
    adapter).

======================================================================
5.0  OTHER TECHNICAL NOTES
======================================================================

This section provides additional technical information and support for
specific uses of Mwave functions and/or applications.

----------------------------------------------------------------------
5.1  Recommendations for Optimum Mwave Modem Performance
----------------------------------------------------------------------

IBM recommends the following settings or conditions for best performance
from your Mwave Modem:

o   For best throughput when sending or receiving data, select the
    highest-ranking available transfer protocol listed here.

    1.  ZMODEM
    2.  Ymodem-G
    3.  TEXT
    4.  ASCII
    5.  XMODEM (only as a last resort)

o   You should enable Hardware Flow Control. Use the Hayes command AT\Q3.

o   Select a modem protocol from this list, with (1) providing the best
    performance, and (6) giving the worst.

        Protocol                   AT Commands use to get protocol
       ------------------------------------------------------------
               1. V.42 / V.42bis              AT\n7"H3
               2. MNP 1-4 / V.42bis           AT\n3"H3
               3. MNP 1-4 / MNP5              AT\n3"H0
               4. V42                         AT\n7"H0
               5. MNP1-4                      AT\n3%C0"H0
               6. non-error corrected         AT\n0

    Refer to the online help available in Mwave Modem for explanation of
    the AT commands required to use one of the above modem protocols.

o   Trouble Connecting at 28.8 kbps

    If you experience difficulties connecting at a modem speed of 28.8
    kbps to a particular number, or if you have trouble connecting to a
    particular modem rotary, try the following.

    -   If the connection is not made and the speaker is OFF:

        1.  Disable V.42 bis and MNP 5 using AT"H%C
        2.  Disable V.42 (AT\N3) or MNP 1-4 (AT\N5). You could also
            disable both with AT\N.

    -   If the connection is not made and the speaker remains on:

        1.  Reduce the maximum modem throughput using the AT commands
            ATS28=18 (for 26400 bps), ATS28=17 (24000 bps), ATS28=16
            (21600 bps), or ATS28=15 (19200 bps).
        2.  If you've tried step 1 and it still does not connect, use
            AT*TH8 to control the speed.

            Once you connect using the AT*TH8 command, remember to reset
            your modem using either AT&F (for factory defaults) or
            AT*TH4. If you forget to reset, your next calls will transmit
            at lower V.34 connection rates.

----------------------------------------------------------------------
5.2  Audio/MIDI Technical Notes
----------------------------------------------------------------------

o   Recording Audio

    Successful recording of audio Wave (.WAV) files depends on a variety
    of factors including processor speed, amount of free disk space, data
    fragmentation on the hard disk, and the type of application used.
    Some computers, particularly those with slower processors, either
    "hang" the system or produce recordings with gaps. These conditions
    occur when using high data rates, such as 44 KHz, which means the
    computer cannot keep up with the data transfer. If you attempt to
    record 44 KHz 16 bit stereo Wave files using a slower PC, you may
    encounter problems.

    Here are some tips that may improve recording:

    -   Erase unnecessary files from your hard disk.

    -   Lower the record rate to 22 KHz or 11 KHz, change to 8 bit,
        and/or change to mono sound. Most applications allow you to
        adjust these parameters.

    -   Use a Hard Disk Defragmentation program (usually included with
        Norton Utilities or Central Point PCTools) to create more contig-
        uous space on your drive. This keeps the slower PC from having to
        work too hard (and take too much time) looking for available disk
        space.

NOTE:  You can use the Disk Defragmentation utility.  Windows 95 includes
this utility under Start/Programs/Accessories/System Tools/Disk
Defragmenter.

    -   If you use a disk compression program (such as DriveSpace,
        DoubleSpace, or Stacker), direct the recorded data to the tempo-
        rary drive created by the compression program or to an uncom-
        pressed drive.  Again, the computer then can process the sound
        without taking the time to uncompress/compress the information.

NOTE:  Windows 95 users can find additional information on the disk com-
pression program DriveSpace under Start/Help/Index/DriveSpace.

    -   Use an alternative audio recording application. Audio programs
        use a variety of techniques to record and playback sound. Some
        may work well in situations where others fail to perform. For a
        basic test, try recording with the Windows Sound Recorder.

----------------------------------------------------------------------
5.3  Sound Blaster Technical Notes
----------------------------------------------------------------------

The "SET BLASTER=" Command

A few games require that DOS uses an environment variable to identify the
location of the sound hardware.  For such games, the following line is
added to the AUTOEXEC.BAT file during installation:

              SET BLASTER=A220 I5 D1

     This parameter...    Tells your game to...
     -----------------    --------------------------------------------
        A220              locate the sound hardware at address 220

        I5                use interrupt level 5

        D1                use DMA channel 1

    These are the default settings created during the installation of
    Mwave.

If you change these settings after installing a new peripheral card, the
"SET BLASTER=..." line must be changed accordingly.

----------------------------------------------------------------------
5.4  Notes about the Mwave Modem
----------------------------------------------------------------------

o   CONFIG.SYS and the Mwave Modem

    Certain configurations of memory managers defined in CONFIG.SYS may
    cause the system to "hang" when loading the DOS modem. This condition
    typically occurs when a memory manager tries to manage upper memory
    and "DOS=UMB" is not set.

    The solution is to always have DOS check for an upper memory manager
    by including DOS=UMB in the CONFIG.SYS file. If DOS uses no memory
    manager, this option has no effect. The DOS Mwave installation auto-
    matically adds this line to your CONFIG.SYS file.

o   V.23/Minitel Modem Connection

    Mwave supports V.23 for modem connection to the Minitel network in
    France only.  V.23 is NOT supported in other countries.

    To use V.23 with your modem application, issue the following AT
    commands:

    -   AT+MS=3 to start a V.23 session
    -   AT&F to end your V.23 session

    In order to use V.23, you must set your communications application to
    the following settings:

    -   7 bit even parity
    -   1 stop bit

    When you start a V.23 modem session, you are limited to V.23 modem
    calls.  However, Mwave still responds with the highest response
    speed, up to V.34.

----------------------------------------------------------------------
5.5  Notes about DOS Mode Support
----------------------------------------------------------------------

Windows 95 does not support Mwave functions if you attempt to access the
Startup Menu by pressing F8 during bootup and then selecting the Command
Prompt Only option.  Windows 95 supports normal Mwave DOS functions
(games, modem, class 2 fax) while in MS-DOS mode or in a Windows 95 DOS
session.
